PORTEKİZ LİMANLARINDA TÜRK BAYRAKLI GEMİLERDE 2022-2026 YILLARI ARASINDA TESPİT EDİLEN EKSİKLİKLER
(Tutulma maddeleri Gri Renkli olarak verilmiştir)

	DENETİM
LİMANI
	DENETİM
TARİHİ
	NO
	REFERANS
	EKSİKLİK

	SETUBAL
	




25.02.2022
	1
	SOLAS CVI R.5
	Maintenance log of Cargo Securing Manual not kept updated (Manual to be reviewed// Minimum lashing material/equipment list not available.

	
	
	2
	SOLAS CIII R.26
	FF lifeboat battery group no.2 out of order// lifeboat engine not able to increase rpm fwd	

	
	
	3
	SOLAS c.III R.16
	RB Davit manual operation out of order (on emergency in case of power failure)

	
	
	
4
	SOLAS/ CII-2 R16
	Engine room ventilation, fire dampers located fwd accommodation- found with hydraulic oil leaks and not closing properly (rubber seal adjustment or out of position)

	
	
	
5
	SOLAS C III  R35
	Training manual not kept updated and a according to LSA equipment installed on board- Rescue boat and davit instructions and FF lifeboat manuals not available)

	
	
	
6
	SOLAS /
C IX / R.3
	Corrective action taken on the ISM system by the Company is required within 3 months. Deficiency(s) marked ISM is (are) objective evidence of a failure, or lack of effectiveness, of the implementation of the ISM Code. The ship will be eligible for reinspection after 3 months from the final date of the report.

	
	





05.08.2024
	1
	SOLAS ch. II-2
Reg. 15.2
	At the time of inspection during the performance of drill (scenario fire on EDG Room), fire team did not perform pre check of equipment. For example pressure inside the two air bottles brought to the drill was bellow 100 bar. Also for example torch was not fitted. New drill to be performed and recorded before departure

	
	
	
2
	ISM
Code / Part A / 1
	Corrective action taken on the ISM system by the Company is required within 3 months. Deficiency(s) marked ISM is fare) objective evidence of a failure, or lack of allociveness, of the implementation of the ISM Code. The ship will be eligible for reinspection after 3 months from the final date of tha report.

	
	
	
3
	MARPOL Annex VI
Reg. 14
	At the time of inspection change over procedures from Company presented were outdated. (ex on SECA still talking about 1 % sulphur content admissible). On recording change over on Engine log book, was miasing completion time, and how this time was calculated, and also recording of compliant fuel on board at that time

	
	
	4
	Ballast Water
Management
	At the time of inspection; both (2) control panel for BVTS were not abble ta scroll down on the curser and check for alarms log: and operation log. Ta be checked and out back into operation

	
	
	5
	MARPOL Annex1
	On IOPP certf. max throughput of the system (OWS) was not shown.

	
	
	
6
	MLC 2006 Title 3
Standard A3.2
	At the time of inspection: emergency opening pus button on both veg room, and cold room beside not working. Also some frost acumulation on door sill was observed; and some buckets on the fiver to collect drainage from the cold unit inside.

	SETUBAL
	07.03.2025
	1
	BWM 2004 / B /
REG. B-2
	During operation it was observed upon checking BWR and crossckecking recorded data on BWMS that operations recorded as a single operation, are in reality diferent and separated operations. As so diferente entries regarding each specific operation have to be observed and recorded. Also inspection took place on the 7th, and there was a operation performed and not recorded on the 6th. That last entrie to be performed on BWRB

	
	
	2
	SOLAS CH.II-2
	During inspection, on the funnel dampers while operating were seized, not closing properly. Operation/test was repeated, maintenance performed, and closing was achieved.


	
	
	3
	MARPOL ANNEX VI
	During inspection while checking Sulphur record book, it was checked the quality for the entries recorded. All the items to be recorded were present, but the duration for each operation was not recorded acordingly. It was not presented or explained how the duration/time from start to completion of any change over was calculated. As from today it was explained on board the use for FOBAS and how to calculate, regarding ship specific inputs namelly ME.


	
	
	4
	SOLAS CH.III
	A fire drill was performed on board (galley). During the witnessing of that drill, the first time it was observed that for example no pre check was performed on COM s, as well for air pressure inside the bottles, before rigging fire man outfit. Also one of the fire team members come to the drill without torch and axe. Drill was then repeated to the satisfaction of its purpose.


	
	
	5
	SOLAS CH.II-1
	During inspection it was observed that shaft generator was out of order. Electric load/capacities and conditions were confirmed for aux 1,2 and 3. Also Class was present on board and acording survey report, the repair for the malfunction due date was established for 20 JUN 25

	
	03.07.2026
	1
	SOLAS ch. V
	PS Gyro Compass not synchronized with main gyro. Service required by Master to the company on 16/06/2026 and Service will be performed at Safi -Morroco.

	
	
	2
	SOLAS ch. V
	STB wiper found out of order.

	
	
	3
	SOLAS ch. Il-1
	Emergency lights on the upper two levels not working, not clearly marked, and rescue boat side projectors out of order

	
	
	4
	BWM
2023 Amendment /
APPENDIX II
	BWRB incorrectly filled between 31/03/2026 and 02/04/2026: Two consecutive full ballast operations were recorded without any corresponding deballasting or sediment disposal operations logged while the vessel was in dry dock in Tuzla.

	
	
	
	
	



	
AVEIRO

	02.07.2025
	1
	SOLAS CH. V
	At the time of inspection the VDR was showing 3 errors: Back Up HDD no connection, DRU no connection and cannot recover DRU and back up HDD. Master informed to send copy of the repair report to PSC office before departure.

	
	
	2
	SOLAS CH. III
	At the time of inspection it was found that the last launching and manoeuvering of FFLB on water was on 24 March 2025.

	
	
	3
	MLC 2006 TITLE 3 / REG. 30.2 STD A3.2
	At the time of inspection it was found that the provisions ran out of fish and the fresh vegetables were also very scarce. There were 19 crew on board and the next port was not known. Master informed to send copy of the delivery note to PSC office before departure.

	
	
	4
	STCW CODE PART A CH. VIII
	At the time of inspection it was noted that the position fixes were not recorded on every watch neither the leaving of Mediterranean ECA area was recorded on the bridge log book. Master instructed to make all relevant records on the log book from now on.


	
	12.05.2026
	1
	SOLAS ch. II-1
	At the time of inspection the Aux. Generator nr 1 was found inoperative. Vessel is fitted with 2 Aux. Generators.

	
	
	2
	SOLAS ch. II-1
	At the time of inspection the battery group nr 2 could not start the EDG

	
	
	3
	SOLAS ch. V
	At the time of inspection the VDR was displayng error 305 - Gyro fault

	
	
	4
	SOLAS ch. II-2
	At the time of inspection a fire-door on a fire class-A division on forecastle was missing.

	
	
	5
	SOLAS ch. II-2
	At the time of inspection a self-closing A- 60 fire door on galley was found permanently trapped open by wire. Another non self-closing fire door on galley - pasage to freezers - was found permantly traped open by rope.

	
	
	6
	SOLAS ch. II-2
	At the time of inspection to self-closing fire doors on emergency escape trunk on ER were found not closing properly

	
	
	7
	MLC 2006 Title 4
	At the time of inspection several floor plates on lower ER deck were found not secured (PSCO almost get injured due to
one unsecure plate)

	
	
	8
	MLC 2006 Title 2
	At the time of inspection it was found that several seafarers (C/O, C/E, 2E, Oiler) have consecutive contracts. Between
these consecutive contracts periods on board were identified with no valid SEAs (ex. 1st contract ending 26 february,
second contract starting 24 march; first contract ending 18 march next starting 24 march). None of the concerned seafarers were disen«mbarked on that missing periods.

	
	
	9
	MLC 2006 Title 4
	At the time of inspection it was found that the safety pins on aft winches were not put in place and one rope on fore mooring was found degradated.

	
	
	10
	ISM Code
	Corrective action taken on the ISM system by the Company is required within 3 months. Deficiency(s) marked ISM is (are) objective evidence of a failure, or lack of effectiveness, of the implementation of the ISM Code. The ship will be eligible for reinspection after 3 months from the final date of the report.

	
	
	
	
	

	LISBON
	23.03.2026
	1
	
	Ship bulb found damage due collision- No report available on board and no classe condition have been issed and apparently the it was not reported to the Company

	
	
	2
	SOLAS ch. V
	Draft marks to be repainted FWD and AFT

	
	
	3
	SOLAS ch. V
	Voyage plan found incomplete on charts and publications in use and performed over publications and charts not updated

	
	
	4
	SOLAS ch. V
	Charts for the Intended voyage from Lisbon to Ravenna to beupdated according to notices to Mariners in accordance with Master requisition

	
	
	5
	SOLAS ch. V
	Nautical Publications for the intended voyage from Lisbon to Ravenna to be updated according to notices to Mariners in accordance with Master requisition (Nautical Almanac, Sailing directions, ALRS, Tide Tables, List of lights, others)

	
	
	6
	SOLAS ch. V
	Echosounder paper -not correctly print depths and paper jammed ad reused

	
	
	7
	SOLAS ch. V
	Magnetic compass found with more than 10 degrees of difference from gyro heading (37/22) and not free moving

	
	
	8
	SOLAS ch. II-2
	Funnel fire flaps not closing properly and operation to open and close to be maintained

	
	
	9
	SOLAS ch. III
	PS and SB davits and boat securing devices not properly maintained and SB lifeboat remote release cable does not follow the boat/ SB lifeboat davit found obstructed with heavy machine and surrounded area with several oil drums (to be dischargedo

	
	
	10
	Load Lines
	Cargo hatch covers securing devices not properly maintained and supports broken (ex: CH1 aft)

	
	
	11
	MLC 2006 Title 4
	SB anchor chain link studs found out of position

	
	
	12
	SOLAS ch. II-1
	Steering gear limit switchs not operational and not correctly adjusted and pump no.2 found under alarm indication

	
	
	13
	SOLAS ch. II-1
	PS embarkation ladder connections and last steps corroded

	
	
	14
	ISM Code
	Corrective action taken on the ISM system by the Company is required within 3 months. Deficiency(s) marked ISM is (are) objective evidence of a failure, or lack of effectiveness, of the implementation of the ISM Code. The ship will be eligible for reinspection after 3 months from the final date of the report.



