BULGARİSTAN LİMANLARINDA TÜRK BAYRAKLI GEMİLERDE 2022-2026 YILLARI ARASINDA TESPİT EDİLEN EKSİKLİKLER
(Tutulma maddeleri Gri Renkli olarak verilmiştir)

	DENETİM
LİMANI
	DENETİM
TARİHİ
	NO
	REFERANS
	EKSİKLİK

	VARNA
	

03.03.2022
	1
	SOLAS ch.II-1 Prt. A
	Emergency towing booklet not as per the ship's specifics.

	
	
	2
	LL AN. I /R.16
	Some quick acting cleats for the hatch covers are missing.

	
	
	3
	MLC 2006 Std.A4.3
	One light in ER inoperative.

	
	
	4
	MLC 2006 Std.A4.3
	El. box for navigation lights on forward mast found broken.

	
	
	5
	MLC 2006 Std.A4.3
	Some floor plates in ER not secured properly.

	
	
	6
	STCW Part Ach.VIII
	Compass error correction not recorded at least once per watch. Deficiency repeated from last PSC inspection 

	
	

23.06.2022
	1
	MLC 2006 Std.A4.3
	Bilge well found with oil residues. Engine room cleanliness is insufficient.

	
	
	2
	SOLAS ch.V R.34
	Missing information R.arding time intervals for ship’s position fixing.

	
	
	3
	MARPOL An.V R.10
	Garbage management plan not ship specific.

	
	
	4
	MLC 2006 Std.A4.3
	Expired medicine found in engine room.

	
	
	5
	STCW Prt. A ch.VIII
	Compass error was not determined at least once per watch. Master instructed.

	
	
27.10.2022
	1
	SOLAS ch.II-1 PartA
	Emergency towing booklet not as per the ship's specifics.

	
	
	2
	SOLAS ch. III R..20
	On some places IMO symbols for LSA were missing.

	
	
	3
	MLC 2006 Std.A4.3
	Rotating parts on one pump in ER were not protected.

	
	
03.03.2022
	1
	BWM Conv.R. B-2
	Ballast record book not filled properly.

	
	
	2
	SOLAS ch. II-1 R.45
	Some electrical mats in ER are missing.

	
	
	3
	MLC 2006 Std A4.3
	Poop deck mooring winch control lever securing device in mid position found broken

	
	
02.05.2023
	1
	MLC 2006 Std A4.3
	Aft mooring station S/S winch control lever securing device in mid position found broken.

	
	
	2
	MLC 2006 Std A3.2
	Portable fridge in galley found without termometer/tempature control.

	
	
	3
	MLC 2006 Std A4.3
	Several pumps in ER rotating parts found not protected.

	
	
	4
	MLC 2006 Std A3.2
	Food in provision stores found not properly segR.ated.

	
	


15.06.2023
	
1
	
SOLAS ch. III R.37
	Muster list did not specify which officers are assigned to ensure that life-saving and fire appliances are maintained in good condition and are ready for immediate use and substitutes for key persons who may become disabledtaking into account that different emergencies may call for different actions.

	
	
	2
	SOLAS ch.III R.17-1
	No any evidence for training and familiarization with the plan found.

	
	
	3
	SOLAS ch. II-2 R.13
	Fire alarms place in ECR monitor appear in Spanish language and crew has to search in separate (translated in Engish) lists the place where the fire is.

	
	
	4
	LL AN. I /R.19
	Goose neck vents on forecastle deck rubber seals found hard and painted.

	
	
24/07/2023
	1
	SOLAS CH II-2/R.14
	Some fire houses not protected.

	
	
	2
	SOLAS CH II/R. 13
	Engine room emergency escape safety rope with belt rigged properly.

	
	
	3
	SOLAS CH III/R.17
	Plans and procedures for recovery of persons from the water are not ship specific.



	VARNA
	

14.09.2023
	1
	SOLAS   CH.V/REG.34
	Passage plan not prepared berth to berth Last two large scale charts BA2286 and SA2287, where is the ship's berth, available OB but not used at al. Courses. WPs not plotted on these charts and ship's position not monitored while ship proceeding with РОВ.

	
	
	2
	MLC/TITLE                 4/STD.A4.3
	Fwd and alt moonng slations wnches, control levors facurina davice a mid position found mesing and where is available found to be frozen.

	
	
07.02.2024
	1
	SOLAS CH.V
	BA2286 chart, where is the ship’s berth, last correction missing.

	
	
	2
	MLC TITLE 4
	Some cf ER floor plates found not fixed by bolts/moving.

	
	
	3
	MLC TITLE 4
	H/C panels found in open position without stoppers.

	
	
09.04.2024
	1
	SOLAS CH. V
	Position fixing interval on passage plan(arrival Varna) not followed by OOW. Master instructed to follow the agreed and approved by him passage plan.

	
	
	2
	SOLAS CH. V
	Entries abt WBTs soundings missing in deck log book for many days.

	
	
	3
	MARPOL ANNEX I
	Entries in ORB for last bunkering not matching the BDN.

	
	

22.10.2024
	1
	STCW
	Compass error not carried out every watch. Master instructed from now to control compass error observation during every nav. watch.

	
	
	2
	MLC 2006
	Bilge water separator pump rotating parts unprotected and unsafe.

	
	
	3
	MLC 2006
	Hatch covers stoppers not in place.

	
	
	4
	SOLAS CH. V
	Deck log book missing entries for daily soundings of tanks. Master instructed to fill the log book from now on.

	
	22.03.2026
	1
	SOLAS ch. V
	International code of signals found not updated.

	
	
	2
	SOLAS ch. IV
	The master is not controlling every day GMDSS logbook. Master instructed to control GMDSS records and operation every day.

	
	
	3
	LSA Code
	All life rafts not marked with port of registry.

	
	
	4
	SOLAS ch. III
	Nobody is checking the necessary arrangements for subsequent abandoning of the ship.

	
	
	
	
	

	
BURGAS

	

08.04.2022
	1
	SOLAS ch.II-2 R.47
	Fire door self-closing device in main vertical zone is not properly adjusted.

	
	
	2
	SOLAS ch.III R.19
	Last emergency drill is not recorded in the ship's log book.

	
	
	3
	SOLAS ch.V, R.28
	Details of the general condition of the ship, such as manning and provisioning, cargo aboard, result of stability/stress checks are not recorded in deck log book

	
	
	4
	SOLAS ch. II-1 R.43
	An emergency light on port side bridge wing is inoperative.

	
	
15.10.2022
	1
	STCW  Sec. A-VIII/1
	Comments in personal records of crew member tables are missing

	
	
	2
	SOLAS ch. V, R.22
	Navigation bridge visibility is obscured at starboard side due to damaged window.

	
	
	3
	 MLC 2006 Title 2
	Watch keeping arrangements are not ship specific.

	
	


25.10.2022
	1
	STCW / Ch VIII
	The std compass error is not determined at least once a watch and, when possible, after any major alteration of course.

	
	
	2
	MLC 2006 Std A4.3
	Dielectric mat in front of main switchboard in engine room, dielectric gloves and shoes are not certified.

	
	
	3
	SOLAS ch. XI, R.9
	Watchman no ID cards checked, no visitor cards provided.

	
	
	4
	COLR. Part C R. 2
	A white Stern light, visible at 3 n.m., showing an unbroken light over an arc of horizon of 135 degrees found inoperative.

	
BURGAS

	
	5
	SOLAS ch. I, R.15
	CSSE Certificate Form E Section 2 Item 9.2 is not properly filledOn board found 2 pcs immersion suitswhich complying with the requirements for life jackets

	
	
10.04.2023
	1
	SOLAS ch.II-2 R.15
	Emergency fire control plan is not up to date.

	
	
	2
	SOLAS ch.V, R.12
	There is alarm on starboard 9GHz radar screen "position sensor lost or invalid”.

	
	
	3
	MLC 2006 Std A4.3
	Auxdiesel generator No1 found with minor leakage of diesel oil.

	
	
	4
	SOLAS ch.II-2 R.14
	Aft starboard engine fire damper cover rubber packing is damaged.

	
	
18.04.2023
	5
	SOLAS ch.II-2 R.7.3
	Heat detector tester is not producing hot air at the appropriate temperature.

	
	
	6
	SOLAS ch. XI-1 R.5
	Continuous synopsis record: 1. Document Number 12, 3, 4, 5 Forms 2, 3 and Document Number 7, 9 Form 3 are missing. 2.Document Number 10, 12 Forms 2 and 3 entries missing.

	
	
	7
	MARPOL An. IV-R.9
	Records for maintenance of STP is missing.

	
	27.04.2023
	1
	SOLAS ch. II-1 R.43
	Two emergency lights on bridge deck and one emergency light on main deck are inoperative.

	
	
	2
	SOLAS ch.V,R.12
	The starboard gyro repeater is not possible to be synchronized with the master gyro compass.

	
	



05.05.2023
	1
	SOLAS ch. II-2R.7
	The fire alarm panel on the bridge indicating general alarm.

	
	
	2
	
ISM Code ch.9- R.3
	Corrective action taken on the ISM system by the Company is required within 3 months. Deficiencies marked ISM is are objective evidence of a failure, or lack of effectiveness, of the implementation of the ISM CodeThe ship will be eligible for reinspection after 3 months from the final date of the report.

	
	
	3
	MLC 2006 Standard A4.3.1
	STBD Side and Port Side hydraulic pipes on the main deck (hatchco amongs) are not property maintained, corrodedMaster instructed for the maintenance accordingly.

	
	
	4
	MLC 2006 Std A4.3
	There is oil in the diesel generator No1 bilges

	
	
	5
	SOLAS ch.II-2 R..14
	Steering Gear and CO2 room air vents (gooseneck) - 2pcs in the AFT area are without fire protecting metal nets.

	
	









20.06.2023
	   1
	SOLAS ch.II-2 R.14
	Emergency fire pump hard to start.

	
	
	   2
	SOLAS ch. III R.20
	Rescue boat engine failed to startBig amount of gasoline leakage was found from the engine.

	
	
	   3
	SOLAS ch. V R.27
	Chart BA 2283 (Maslen Nos to Nos Kaliakra) is missing.

	
	
	   4
	SOLAS ch.III R.16
	Rescue boat davit limit switch is inoperative.

	
	
	   5
	SOLAS ch. V 
	STBD Side Pilot Ladder is not in accordance with IMO Res. A.1045(27)

	
	
	   6
	ISPS Code Part A/7
	Watchman no visitor card provided.

	
	
	   7
	MLC 2006 Std A3.1
	Air condition is out of order.

	
	
	   8
	MLC 2006 Std A3.2
	Two deep freezers thermometers are found inoperative.

	
	
	   9
	COLR. / Rule 20
	Masthead lights inoperative.

	
	
	 10
	MARPOL An. I-R.17
	Oil record book Part I found with wrong records for bilge and sludge tanks. Changing Lub. oil of Auxiliary engine No.1,2 and3 not recorded in Oil Record

	
	
	  11
	SOLAS ch. II-2 R.14.1
	CO2 room and Paint Store vent covers - 2pcs are not properly maintainedRubber gaskets are in poor condition, missing and fire protecting metal nets are missing.

	
	
	  12
	SOLAS ch.II-2 R.12
	Tester for heat detector is not producing hot air at the appropriate temperature.

	
	
	  13
	MLC 2006 Std A4.3
	Oil leakage.

	
	
	  14
	MLC 2006 Std A4.3
	Covers/Lights-5/11pcs in accommodation, forepeak and engine room are cracked / inoperative, missing

	
BURGAS
	
	  15
	SOLAS ch. II-1 R.26
	Main Engine found with water leakage

	
	
	  16
	ISM Code ch.IX / R.3
	Safety management audit by the Administration is required before departure of the ship. Deficiencies marked ISM are objective evidence of a serious failure, or lack of effectiveness, of implementation of the ISM Code.

	
	
	  17
	MARPOL An. IV-R.9
	Type approved certificate for Sewage treatment plant is not presentedRecords for maintenance are missing.

	
	
	  18
	MLC 2006 Std A4.3
	Permit to work system is not as required. Risk assessment are presented only.

	
	
30.10.2023
	   1
	SOLAS/ch.V
	The standard magnetic compass liquid is with a big air bubble.

	
	
	   2
	SOLAS/ch. II-2/r.14
	One heat detector cover in the accommodation is damaged.

	
	
	   3
	SOLAS/ch.II-2/r.14
	A heat detector tester is not approved type.

	
	
	   4
	MLC 2006 Title 3
	A meat freezer thermometer is missing.

	
	


02.01.2024
	 1
	SOLAS CH. V
	Chart BA 2283 is missing.

	
	
	 2
	SOLAS CH.II-2
	Fire control plan is not up to date. Missing info regarding flame detectors.

	
	
	 3
	MLC 2006 TITLE 4
	Certificates for dielectric mats in front of engine room main switchboard, emergency diesel generator switchboard are not presented.

	
	
	 4
	ICLL 2006
	Scupper pipe inlets-5 pcs on deck, protecting nets are missing.

	
	
	 5
	MARPOL AN. V
	Big amount of garbage found stored on deck aft side.

	
	01.02.2024
	   1
	ICLL ANNEX ı R.12
	Superstructure waterlight doors -2pcs of deck Fire store and Air condition room are with spots of corrosion.

	
	
	   2
	MLC TITLE 4
	Deck lighting -3pcs are inoperative.

	
	



23.07.2024
	1
	COLREG/PART C/RULE 20
	Masthead lights are inoperative.

	
	
	2
	SOLAS CH. II-2
	Battery room, Bridge store and Deck Bosun store watertight fire doors are corroded.

	
	
	3
	SOLAS CH II-1
	Main Engine failed to work. Under repair. Not spare parts on board. It waiting

	
	
	4
	MARPOL ANNEX VI
	Incinerator found out of order. Under repair. Port authorty was not informed accordingly.

	
	
	5
	BWM REG. D-2
	BWMS found out of order. Port authority was not informed accordingly. New IBWMCertificate was issued.

	
	
	6
	ANTİ FOULING SYSTEMS ANNEX 4
	Found International Anti-fouling-System Certificate on board with previous vessel name - Zeynep Ka, issued by Bureau Veritas.

	
	
	7
	ISM CODE-SOLAS CH.IX/REG.3
	Corrective action taken on the ISM system by the Company is required within 3 months. Deficiencies marked ISM are objective evidence of a failure, or lack of effectiveness, of the implementation of the ISM Code. The ship will be eligible for reinspection after 3 months from the final date of the report.

	
	
02.09.2024
	1
	MLC 2008 Tite 4
	Dielectric mat in front of engine room main switch board and dielectric gloves, and shoes are not certified.

	
	
	2
	ICLL  / ANNEX A	
	Watertight window - 7pcs in accommodation, rubber gaskets are in poor condition.

	
	

31.03.2025
	1
	SOLAS CH.II-1
	Steel insulation of Main engine exhaust pipe is damaged and not fixed properly in a few areas.

	
	
	2
	SOLAS CH.II-1
	Insulation of turbocharger turbine sides on both Auxiliary engines No.1 and 2 are missing.

	
	
	3
	SOLAS CH. III
	Instructions for rescue boat including stowage and securing is not included in SOLAS training manual.

	
	
	4
	SOLAS CH. V
	Last record in compass correction log is from 12.03.2025.

	
	20.05.2025
	1
	MARPOL ANNEX I
	15ppm calibration certificate is expired.

	
	
	2
	MLC 2006 TITLE 4
	Engine room emergency exit safety harness is missing.

	
BURGAS


	26.09.2025
	1
	SOLAS CH. V
	GMDSS Manual is old edition.

	
	
	2
	MLC 2006 TITLE 4
	Por Side AFT area one mooring rope is in poor condition.

	
	
	3
	SOLAS CH. V
	Compass observantion book plan last entry 01.07.2025. Master instructed accordingy.


	
	03.12.2025
	1
	SOLAS CH. II-1
	Seat of drain plug for the vents drip tray of Diesel oil bunker tanks No.1 and 2 is corroded and drip tray cannot be plugged. Also some holes are observed on the mashroom of the Compressor room exhaust fan.

	
	
	2
	ISM CODE / SOLAS 99/00 AMEND CH. IX / EG. 3
	Corrective action taken on the ISM system by the Company is required within 3 months. Deficiencies marked ISM are objective evidence of a failure, or lack of effectiveness, of the implementation of the ISM Code. The ship will be eligible for reinspection after 3 months from the final date of the report.

	
	
	3
	MARPOL ANNEX VI
	Black smoke noticed continuously coming out from Aux. Boller. (confirmed by Ch. Engineer). Vessel not comply with SEEMP.

	
	
	4
	SOLAS CH. II-1
	Aux. Engine No2 Fresh water cooling pipe found temporary repaired by metal plastic.

	
	
	5
	MLC 2006 TITLE 4
	Dangerous area around high voltage antena on the monkey Bridge is not marked properly.

	
	
	6
	SOLAS CH. II-1
	Main Engine found water leakage from unit No1

	
	
	7
	MLC 2006 TITLE 4
	Found many oily rage between pipes of main engine.

	
	

14.01.2026
	1
	SOLAS Ch. II-1 Reg.26
	Local fuel oil pressure gauge of Auxiliary engine is not running and standing by.

	
	
	2
	SOLAS Ch. II-2 Reg.16
	Wire mesh ventilation of the fire locker is obstructed by dirt.

	
	
	3
	SOLAS Ch. II-2 Reg.14.1
	Fire hydrant on bridge port side is leaking during test of emergency fire pump.

	
	
09.02.2026
	1
	SOLAS Ch.V Reg.34
	Voyage plan from Guluc to Burgas is not berth to berth.

	
	
	2
	STCW Code Part A ch.VIII
	Voyage plan is not updated with anchor position. Psn fixes are not approved as per passage plan.

	
	
	3
	BWM Conv. Annex  Reg.B1
	Ballast water management plan is not updated with D2 method. There is still references with D1 method.

	
	
	4
	SOLAS Ch.II-1 Reg.27
	Several electric cables isolation in the way of bridge deck are cracked/wasted.

	
	23.02.2026
	1
	SOLAS CH. II-2
	One EEBD at the entrance of the E/R found with insufficient pressure of

	
	
	2
	MARPOL ANNEX I
	Number of F.O. bunker and other drip trays on deck are not provided with plugs

	
	
	3
	SOLAS CH. V
	Passage plan from Samsun to Burgas is not updaled with anchor position

	
	
	4
	MARPOL ANNEX I
	International standard discharge connection is rusty and not as per the
MARPOL Annex 1 requirements. Also the IMO symbol on its box is painted and deteriorated.

	
	
	5
	SOLAS CH. VI
	MSDS's are missing for the F.O bunker received on 17.02.2026 in Samsun and for the lube oil bunker received on 04.12.2025 in Tuzia

	
	05.05.2026
	1
	SOLAS ch. XI-1
	Original CSR No.9 is not presented on board.

	
	
	2
	IBC Code
	The original ship's certificate for carrying of Dangerous Chemicals in Bulk (ICoF/IBC
Code) is not presented on board.

	
BURGAS

	
	3
	SOLAS ch. V
	Safety contour set below safety depth.

	
	
	4
	SOLAS ch. II-2
	The emegency exit from E/R is not provided with safety rope and safety hamess-

	
	
	5
	MLC 2006 Title 3
	Broken and missing tiles are observed on the floor of the ship's Galley. Also the lower part of the door frame in way of the provision stores is corroded.

	
	
	6
	MARPOL Annex VI
	In the International Energy Efficiency Certificate under position 7.1 is marked that the vessel is provided with SEEMP, although the ship does not require such plan.

	
	10.07.2026
	1
	COLREG Rule 20
	Stand by aft mast head light is inoperative.

	
	
	2
	SOLAS Ch.VI Reg.5.1
	MSDS’s of all lubricants stored in the engine room store room next to steering gear compartment are not presented.

	
	
	3
	MLC 2006 Title 4 Std.A4.3
	All 4 (four) portable platforms/staging located next to each of the Auxiliary engines No1,2,3 and 4 are not properly fixed/secured and hazardous for the ship’s crew.

	
	
22.09.2026
	1
	SOLAS Ch IV Reg.7.1.5
	Satellite EPIRB is not marked with ship’s name, mmsi, call sign.

	
	
	2
	SOLAS Ch III Reg.20
	Several lifebuoys marking of ship name, port of registry are wasted and not readable.




