KANADA LİMANLARINDA TÜRK BAYRAKLI GEMİLERDE 2022-2026 YILLARI ARASINDA TESPİT EDİLEN EKSİKLİKLER
(Tutulma maddeleri Gri Renkli olarak verilmiştir)
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28.02.2023
	1
	SOLAS CII-1 R13
	At the time of the inspection one engine room double bottom tank sounding pipe was found not self-closing

	
	
	2
	ICLL An.I R. 12
	At the time of the inspection the door in fore castle missing gasket

	
	
	3
	SOLAS Ch.II-1 R.44
	At the time of the inspection the emergency light is not working at lifeboat

	
	
	4
	SOLAS Ch.II-1 R.43
	At the time of inspection the emergency generator failed twice to come up on load automatically during black-out

	
	
	5
	SOLAS Ch.II-1 R.37
	At the time of inspection the telephone bell and strobe were inoperative by the main engine local control stand.

	
	
	6
	SOLAS Ch.IV / R.4
	At the time of inspection the navtex is not working

	
	
	7
	SOLAS Ch.II-2 R.9.4
	At the time of inspection two A-60 Fire doors (at upper engine room entrance and in lower engine room escape trunk) were not self closing and not closing tight.

	
	
	8
	SOLAS Ch.II-2R.10.3
	At the time of inspection multiple portable and dollied fire- fighting extinguishers in the engine room and in galley are missing their seals/tags ; to be re-certified accordingly.

	
	
	9
	COLREG Rule 20 
	The nuc light is not working 

	
	
	10
	SOLAS Ch.V Reg.27
	The publication STCW is not on board

	
	
	11
	SOLAS Ch.V Reg. 14
	Actual workin language is Turkish but in the ship board policy is English

	
	
	12
	SOLAS Ch. III R.20
	The rescue boat’s fuel oil tanks were both found half-filled and the starboard becketed line was found wasted. 

	
	
	13
	SOLAS Ch.II-1 Part C,D,E,F, R.26
	Auxiliary Engine No.1 was found in operative, shutting down automatically a few seconds after being started. Flag dispensation from the Administration must be issued to cover this condition.

	
	
	14
	SOLAS Ch.II-PartR.4
	The bilge is not working

	
	
	15
	SOLAS Ch.II-1 R.31
	Vessel found in dead ship condition after black out

	
	
	16
	MARPOL An.I R.14
	The crew was unable to demonstrate the operational readiness of the oily water seperator and its 15 ppm audible/visual alarm

	
	
	17
	MARPOL An. IV R.9
	Sewage treatment plant was showing an abnormal alarm

	
	
	18
	ISM Code Ch.IX R.3
	Safety management audit by the Administration is required before departure of the ship. Deficieny(s) marked ISM is objective evidence of a serious failure or lack of effectiveness

	
	
	19
	MLC 2006 R.3.1
	Three toilets on the main deck’s crew’s water closets : one is running constantly, one is obstructed by many garbage bags, and two of them have their flush mechanism’ handle broke

	
	
	20
	MLC 2006 St.3.1
	Due to total loss of power of vessel sanitary and living conditions are below minimum standard in Canadian winter conditions.

	
	
	21
	SOLAS, STCW, MLC 2006
	Master instructed that inspection is suspended due to the actual condition of the ship and its equipment, also taking into account the crew’s living andworking conditions The inspection will resume after the flag and R.O. have ensured that the ship complies with all the relevant conventions.

	CONTRECOEUR
	30.03.2026
	1
	SOLAS CH III
	The previous enclosed space drill, registered in the deck log book was did not have a enclosed space work permit issued as reference as required.

	
	
	2
	SOLAS ch. II-2
	The self-closing fire doors to the engine room from main deck and from the steering gear room were not latching.

	
	
	3
	SOLAS ch. II-2
	The quick closing valve was not functional with the actuator dismantling itself during testing.

	
	
	4
	COLREG
	The entire portside navigation lighting was found to be inoperative.

	
	
	5
	MARPOL Annex I
	The oily water separator was found inoperative.

	
	
	6
	MARPOL Annex I
	The oily water separator (OWS) was found inoperative. A new Condition was issued by the RO as The defective control valve for sample FW of 15 ppm sensor is to be rectified by the due date (Ref: Flag dispensation email of 02 April 2026)". DUE DATE: 01 June 2026. Short term IOPP was issued valid until 1 June 2026.

	
	
	7
	ISM CODE
	Safety Management Audit by the Administration is required before departure of the ship. Deficiencies marked ISM are objective evidence of a serious failure or lack of effectiveness of the implementation of the ISM Code.
Corrective Action taken in the ISM system by the Company is required within 3 months. Deficiencys) marked
ISM is (are) objective evidence of a failure, or lack of effectiveness, of the implementation of the ISM Code. The ship will be eligible for reinspection after 3 months from the final date of the report

	
	
	8
	MLC 2006 TITLE 3
	The ship machinery spaces, including engine room, steenng gear room, chemical locker were found dirty and in need of cleaning and making the space more tight.

	
	
	9
	MLC 2006 TITLE 4
	The chemical suits were missing in the chemical room.

	
	
	10
	MLC 2006 TITLE 4
	No incident report nor investigation were completed on board for the injured suffered by the fitter as per photos and medical reports provided.

	VANCOUVER
	




22.01.2025
	1
	SOLAS ch. II-2
	Galley fire damper not readily accessible and not closing effectively.

	
	
	2
	SOLAS ch. II-2
	Anti-splash tapes on fuel high pressure connections, missing for several machineries.

	
	
	3
	SOLAS CH V
	Tidal stream information for arrival passage not taken into account effectively.

	
	
	4
	MARPOL Annex I
	Manually operated 3 way valve inoperative/ seized at the time of testing Oil Filtering Equipment.

	
	
	5
	MARPOL Annex V
	Food waste storage in provision refrigerated chambers, not in accordance with garbage management plan.

	
	
	6
	BMW ANNEX REG B-2
	Ballast water record book not completed for ballast operations conducted in port

	
	
	7
	ISM Code, SOLAS
	Corrective action on the ISM system taken by the company is required within 3 months. Deficiencies marked ISM are objective evidence of a failure, or lack of effectiveness of the implementation of the ISM Code.

	
	
	8
	ISPS CODE PART A/7
	Access control to vessel not effectively maintained.

	
	





08.09.2026
	1
	MLC 2006 Title 2
	Crew not being paid as per their CBA.

	
	
	2
	LOAD LINES
	Hatch cover resting blocks wasted and they are resting on the coaming.Def. to be attended with in 90 days.

	
	
	3
	SOLAS Ch. II-1 Reg. 3-4.2
	At time of inspection watch keepers not familiar with the ETA deployment procedures and not aware of the tools usage.

	
	
	4
	SOLAS Ch. V
	On board declared language is English.Few crew members speaks only Turkish (Turkish) and few only speaks English (Filipino).

	
	
	5
	SOLAS Ch. II-1 Reg. 26
	Engine room gauges few places leaked out, foggy, non readable, inclusive of
A/E's. Def. to be attended with in 90 days.

	
	
	6
	MARPOL Anx I Reg.14
	Ship staff unable to carry out testing of OWS safety valve.

	
	
	7
	
ISM Code
	Corrective action taken on the ISM system by the Company is required within 3 months. Deficiency(s) marked ISM is (are) objective evidence of a failure, or lack of effectiveness, of the implementation of the ISM Code. The ship will be eligible for reinspection after 3 months from the final date of the report.

	
	
	8
	MLC 2006 Title 1
	Training officers official training records books not filled. Blank copies available on board.



