İSPANYA LİMANLARINDA TÜRK BAYRAKLI GEMİLERDE 2022-2026 YILLARI ARASINDA TESPİT EDİLEN EKSİKLİKLER
(Tutulma maddeleri Gri Renkli olarak verilmiştir)

	DENETİM
LİMANI
	DENETİM
TARİHİ
	NO
	REFERANS
	EKSİKLİK

	CEUTA
	
28.06.2022
	1
	MLC 2006 Std A3.2
	Messroom floor dirty.

	
	
	2
	MLC 2006 Std A3.2
	Galley floor and hood dirty.

	
	
	3
	ILO Conv.147/92
	Common toilet, dreinage pipe from washing basin holed flooding to restroom.

	
	




28.07.2026
	1
	Solas ChV Rule 23
	Pilot ladder broken when pilot disembarking.

	
	
	2
	Solas Ch III Rule 29
	Local emergency steering operation.Lack of knowledge.

	
	
	3
	Solas Ch III Rule 16
	L/B sbs davit stuck.Impeding to lower boat to water.Rectified but to be maintaned.

	
	
	4
	Lsa Code Ch IV Rule 4.4
	Sbs L/B hull defense damaged/destroyed after accidentally lowering to water.Work must done by an approved service company.

	
	
	5
	Solas Ch III Rule 16
	Remote operation wire broken.

	
	
	6
	
Solas Ch IX Rule 3
	Corrective action taken on the ISM system by the Company is required within 3 months. Deficiency(s) marked ISM is (are) objective evidence of a fallure, or lack of effectiveness, of the implementation of the ISM Code. The ship will be eligible for reinspection after 3 months from the final date of the report.

	
	

03.09.2026
	1
	AFS Conv.
	AFS certificate information Organotin and Cybutryne are missing.

	
	
	2
	Marpol A.VI
	IEE certificate information (EEDI and EEXI) are missing.

	
	
	3
	SOLAS ch.III R.37
	Alarm signals are not indicated.Person for maintenance LSA&FF missing.

	
	
	4
	SOLAS ch.III R.19
	Last time rescue boat lowered to the water dated in March 2026.

	
	
	
	
	

	CARTAGENA

	

17.11.2022
	1
	SOLAS ch.II-1-R.26
	Emergency generator not working properly 45 minutes for starting.

	
	
	2
	LL B/I/II
	Steering gear door closing devices not working properly.

	
	
	3
	LL Reg.6.6
	Disc Plimsol marks no readable (next dry dock).

	
	
	4
	LL Reg.22-22.1
	Port side hull areas found rusty.

	
	
18.11.2022
	5
	SOLAS ch.II-2 R.10
	Hose connection C.I water leaks.

	
	
	6
	SOLAS ch.II-2 R.7.1
	Smoke detector engin control room not working properly.

	
	
	7
	SOLAS ch. II-1 R.44
	230 volt emergency busbar shows lack of insulation due electrical derivation on lighting in forecastle.

	
	
	
	
	

	ALICANTE
	

13.06.2023
	1
	SOLAS ch.II-2-R.15
	Lack of training and familiarity in the fire drill

	
	
	2
	SOLAS ch.IIIR.19
	Lack of training and familiarity in 'the abandon drill

	
	
	3
	MLC 2006S td.A4.3
	Main switch board restricted access.

	
	
	4
	STCW PartA/VIII/I
	The drills hours are not recorded on Daily working hours.

	
	
	
	
	

	ALGECIRAS
	

28.04.2023
	

1
	


SOLAS ch. III 
	

Found portside lifeboat engine did not start. After change of batteries it worked properly. 

	
	
	
	
	

	ALMERIA
	

24.10.2023
	1
	ISPS CODE/PART A.7
	No security access control to ship was establised when the PSCO arrived. Master instructed to comply with ship security plan.

	
	
	2
	MARPOL/R.17
	Wrong entry in the ORB. Item code 11 weekly inventory instead of code 12 (transfer). The captain didn't sign the ORB.

	
	
	3
	SOLAS/R.14.1
	The fire main line had a leakage on deck.

	
	
	4
	MLC/TITLE 4
	Paint stole switchboard light inoperative.

	ALMERIA
	




24.10.2023
	5
	SOLAS/CH. II-2/R.14.1
	During the fire drill one crew member left a lit cigarette on the deck, close to oil drums. The crewmember dressed with the firemanoutfit forgot the torch and to wear correctly the helmet. Master intructed to perform more drills to improve crew familiaritation.

	
	
	6
	ISM CODE/PART A/1
	Corrective action taken on the ISM system by the Company is required within 3 months. Defİciency(s) marked lSM is (are) objective evidence of a failure, or lack of effectiveness, of the implementation of the lSM code. The ship will be eligible for reinspection afler 3 months from the final date of the report.

	
	
	7
	SOLAS/R.14.1
	Emergency escape trunk in the engine room was obstructed and not ready for use.

	
	
	8
	MLC/TITLE 3
	The hospital was dirty and not ready for use due to some goods were stored inside.

	
	
	9
	SOLAS/CH. II-2/R.14.1
	CO2 alarm could not be heard in the engine room. Master instructed to keep fixed fire extinguising installation ready for use.

	
	
	10
	MLC/TITLE 4
	Oil leakage from windlass pump system on the fore castle.

	
	
	11
	MLC/TITLE 4
	There were traces of paint and water on the deck ofthe paint store.

	
	
	
	
	

	TARRAGONA
	

11.01.2024
	
1
	STCW PART A ch.III
	
4th Engineer Coc is power limited up to 3000 kW

	
	
	
2
	SOLAS CH.V
	
Charts were not updated. Rectified during the inspection.

	
	
	
	
	

	
SEVILLA
	

02.04.2024
	1
	MLC 2006 
	The MF/HF antenna area must be protected and posted a symbol of high voltage.

	
	
	2
	SOLAS CH. III
	The instructions of the hook for launching the rescue boat/life raft must be posted (under emergency light)

	
	
	
	
	

	
CABEZUELA
	





17.05.2024
	1
	SOLAS CH. II-1
	EMERGENCY GENERATOR INOPERATIVE

	
	
	2
	SOLAS CH. V
	AIS SHOWING WRONG OWN DATA: POSITION ERROR OUT OF RANGE. HEADING READING MISSING

	
	
	3
	SOLAS CH. V R.19
	GPS POSITION ERROR OUT OF RANGE

	
	
	4
	MLC / TITLE 4R.4.3
	STARBOARD ANCHOR NOT PROPERLY STOWED IN HAWSEPIPE

	
	
	5
	STCW VIII
	NO OFFICER FROM THE ENGINE DEPARTMENT ON BOARD WHEN PSC ARRIVED TO THE SHIP

	
	
	6
	SOLAS CH. IV
	MH/HF SELF TEST - UNABLE TO COMPLETE THE TEST

	
	
	7
	SOLAS CH. IV
	INMARSAT LINK TEST - UNABLE TO PERFORM THE TEST

	
	
	8
	SOLAS CH. IV
	CREW UNABLE TO TEST MH/HF & INMARSAT EQUIPMENT USING THE RESERVE SOURCE OF ENERGY

	
	
	9
	SOLAS CH. III
	RESCUE BOAT SEARCH LIGHT INOPERATIVE

	
	
	
10
	
SOLAS C IX
	BILGE WATER DRAIN TANK RECENTLY CLEANED BY CREW BUT NO ENCLOSE SPACE ENTRY PERMIT ISSUED.
MASTER INSTRUCTED TO IMPROVE ENCLOSED ENTRIES DRILLS

	
	
	11
	MARPOL ANNEX I
	ORB WRONG ENTRIES (OIL RESIDUES DISCHARGES, OILY WATER TRANSFER, ETC.)

	CABEZUELA
	
	12
	SOLAS CH. II-1
	BILGE WATER DRAIN TANK - MANHOLE COVER NOT FULLY

	
	
	13
	SOLAS CH. II-1
	DECK BENEATH OILY WATER SEPARATOR HOLED

	
	
	
14
	ISM CODE- SOLAS 99/00 AMEND / IX/REG. 3
	Corrective action taken on the ISM system by the Company is required within 3 months. Deficiency(s) marked ISM is (are) objective evidence of a fallure, or lack of effectiveness, of the implementation of the ISM Code. The ship will be eligible for reinspection after 3 months from the final date of the report.

	
	
	15
	MLC 2006 / REG.4.3
	ALARM INSIDE REFRIGERATION CHAMBERS OUT OF ORDER

	
	
	
	
	

	GIJON
	09.04.2026
	1
	Load Lines
	Bosun Store Vent Closing device missing (159 mm diameter aprox close to entrance door)

	
	
	2
	MARPOL Annex V
	To instruct the crew how to segreate propertly the waste (crew messroom dedicated bin for food full of plastics)

	
	
	3
	SOLAS ch. II-2
	Several vent closing devices not marked

	
	
	4
	SOLAS ch. IlI
	Most suits are XL size (over 190 cm height) while crew members are shorter

	
	
	5
	SOLAS ch. V
	ALDIS light inoperative with emergency battery

	
	
	6
	SOLAS ch. VI
	The unloading of the vessel was carried out not following the unloading plan

	
	
	7
	SOLAS ch. VI
	Fire fighter no familiar with the use of SCBA on board

	
	
	8
	ISM Code
	Corrective action taken on the ISM system by the Company is required within 3 months. Deficiencies marked ISM are objective evidence of a failure, or lack of effectiveness, of the implementation of the ISM Code. The ship will be eligible for reinspection after 3 months from the final date of the report.

	
	
	9
	SOLAS ch. VI
	Ship shore safety checklist not readily available.






