HIRVATİSTAN LİMANLARINDA TÜRK BAYRAKLI GEMİLERDE 2022-2026 YILLARI ARASINDA TESPİT EDİLEN EKSİKLİKLER
(Tutulma maddeleri Gri Renkli olarak verilmiştir)

	DENETİM
LİMANI
	DENETİM
TARİHİ
	NO
	REFERANS
	EKSİKLİK

	
SPLIT

	

19.02.2022
	1
	SOLAS ch.IV R.7
	Navtex printout bearly readible. Message from Split Radio station is missing. 

	
	
	2
	SOLAS ch.V R.27
	BA CHART 269 last two updates missing.

	
	
	3
	SOLAS ch. III R.20
	ITU list IV Edition 2019 found on board. NP47 not included voyage plan to Split.

	
	
18.03.2022
	1
	SOLAS ch.V R.27
	ITU list IV Edition 2019 found on board.

	
	
	2
	SOLAS ch. II-2 R.45
	Emergency Escape doors in E/R not closing properly.

	
	


13.02.2023
	1
	SOLAS ch.IV R.4
	Navtex not set to receiving from Adriatic region (Letter Q)

	
	
	2
	SOLAS ch. III R.32.2
	Two life jackets light on navigation bridge expired on 09/2022.

	
	
	3
	MLC 2006 Std A3.1
	Galley ventilation hood greasy.

	
	
	4
	MLC 2006 Std A4.3
	Grinder/wire brush machine in E/R missing.

	
	
29.03.2023
	1
	SOLAS ch. III R.20
	Rescue boat engine running in period less than 3 min.

	
	
	1
	SOLAS ch.IV R.4
	Navtex device not received from Split radio. Not selected (Letter Q).

	
	
	
	
	

	RIJEKA
	






29.08.2023
	1
	SOLAS CH II/R.14.2
	Self closing doors in galley can not be closed. Closing arm is broken and locking mechanism is not working. CO2 protecetd paint locker doors can not be cosed.

	
	
	2
	SOLAS CH.V/R.27
	Rijeka port (BA chart 2719), Rijeka approach (BA chart 1996) and Kvarner area (BA chart 202) are missing. Vessel was in Rijeka port two weeks ago.

	
	
	3
	SOLAS CH.V/R.34
	Route not plotted on nautical charts. Positions not plotted on nautical chart.

	
	
	4
	ICLL AN. I/R.15
	Several cleats on hold No. 1 and hold No.2 are missing or are damaged

	
	
	5
	COLREG/RULE 20
	Both stern anchor lights are not working

	
	
	6
	SOLAS/II-1/R.26
	Rescue boat emergency light not working

	
	
	
7
	ISM CODE-SOLAS/IX/R.3
	Corrective action taken on the ISM system by the Company is required within 3 months, Deficiency(s) marked ISM is (are) objective evidence of a failure, or lack of effectiveness, of the implementation of the ISM Code.The ship wil be eligible for reinspecton after 3 months from the final date of the report.

	
	
	8
	SOLAS/R.19
	Fire drill in galley failed.

	
	
	9
	ICLL/R.23
	Watertight window in oiler's cabin which is situated on main deck is leaking water

	
	
	10
	MLC/STD. A4.3
	Common bathroom door frame is corroded with sharp edges on door's treshold.

	
	
	11
	MLC/STD A3.1
	Oiler’s cabin on upper deck floor found damaged with holes

	
	

07.10.2024
	1
	MLC 2006
	Quantity of fresh fruit and vegetables is not sufficient for next voyage.

	
	
	2
	SOLAS CH.II-2
	Spare charges for fire extinguishers are not according to regulation regarding quantity. Spare extinguishers for life boats are missing.

	
	
	3
	SOLAS CH.II-2
	Isolation valve on top of cargo tank no.6 is not closing properly.

	RIJEKA
	
	4
	SOLAS CH. III
	Lite boats were not maneuvered in water In proper intervals. Last two drills tack place on 10.5.2024, and 19.9.2024, which is more than three month period requirement. There are no records that boats were maneuvered in water but it is only recorded that boats were to sea level.

	
	
	5
	SOLAS CH. II-2
	Port side flooding dumper in pump room can not be opened fully by remote means.

	
	
	6
	
ISM CODE
	Corrective action taken on the ISM system by the Company is required within 3 months. Deficiency(s) marked ISM is (are) objective evidence of a failure, or lack of effectiveness, of the implementation of the ISM Code. The ship will be eligible for reinspection after 3 months from the final date of the report.

	
	11.03.2025
	1
	SOLAS CH.III
	No evidence that rescue boat was maneuvered in water in last three months

	
	
	2
	ISPS CODE
	There is no evidence that ISPS exercise was carried out in required intervals

	
	
	3
	ISPS CODE
	Access doors on superstructure found unlocked

	
	
	4
	SOLAS CH.II-2
	Selclosing fire doors found blocked in open position: ECR and steering gear room.

	
	
	5
	SOLAS CH.I
	Ship type on Cargo ship safety construction certificate is different from ship type on SMC.

	
	
	6
	
ISM CODE-SOLAS 99/00
	Corrective action taken on the ISM system by the Company is required within 3 months. Deficiency(s) marked ISM is (are) objective evidence of a failure, or lack of effectiveness, of the implementation of the ISM Code. The ship will be eligible for reinspection after 3 months from the final date of the report.

	
	
	7
	SOLAS CH.II-2
	Isolating valves on fire line are hart to operate.

	
	





26.11.2025
	1
	SOLAS ch. II-2
	Several self closing fire doors (D/G room , A/C room ) found in blocked in open position.

	
	
	2
	SOLAS ch. II-2
	ME FO service tank quick closing valve found secured in open position.

	
	
	3
	SOLAS ch. II-1
	UMS alarms not transmitted in engineers cabins. Ship is classed as UMS and MSMD is stating periodically unattended
machinery. Engineers watch is maintained at all times.

	
	
	4
	MLC 2006 Title 4
	Rotating parts protection on shaft generator missing.

	
	
	5
	MARPOL Annex I reg. 12
	20 cm of oily water found below M/E

	
	
	6
	SOLAS ch. III
	Control wire for lowering of lifeboat from inside broke during lowering

	
	
	7
	SOLAS ch. XI-1
	CSR no.9 wrong year stated on certificate

	
	
	8
	MLC 2006 Title 3
	Shower hose is missing.

	
	
	9
	COLREG/ Part C /
RULE 20
	One must head navigational light and one NUC light not working

	
	
	10
	MLC 2006 Title 3
	Fresh fruit quantity not sufficient for next voyage.

	
	
	11
	
ISM Code
	Corrective action taken on the ISM system by the Company is required within 3 months. Deficiency(s) marked ISM is (are) objective evidence of a failure, or lack of effectiveness, of the implementation of the ISM Code. The ship will be eligible for re inspection after 3 months from the final date of the report.

	
	
	
	
	





	BAKAR
	06.05.2026
	1
	SOLAS ch. II-2
	Emergency generator exhaust pipe spark arresting mesh is broken.

	
	
	2
	SOLAS ch. III
	FF LB was last time lowered and maneuvered in water on 23 oct. 2025. which is more than required three month interval

	
	
	3
	SOLAS ch. III
	Self contained air bottles found empty.

	
	
	4
	SOLAS ch. III
	Rescue boat davit not ready for use in emergency mode. Pressure bottles found empty. Crew couldn't operate davit.

	
	
	5
	SOLAS ch. III
	Fire drill in emergency generator failed Crew attacked fire with short hose, fire teams. were with wrong composition according to muster list, muster place was provisional (not on C deck), aft ventilation not closed, quick closing valve not operated.

	
	
	6
	STCW Code Part A
	Crew is not able to operate rescue boat davit.

	
	
	7
	ISM Code
	Corrective action taken on the ISM system by the Company is required within 3 months. Deficiencys) marked ISM are objective evidence of a failure, orlack of effectiveness, of the implementation of the ISM Code. The ship will be eligible for reinspection after 3 months from the final date of the report.

	
	
	8
	BWM
2004 / D / Reg. D-2
	Ballast water treatment is alarming big number of non compliant operations due to low UV intensity.

	
	
	
	
	

	
PLOCE

	


08.07.2026
	1
	MLC 2006 Title 3 Std. A 3.1
	The extraction duct of the hood in galley found dirty due to fat residue.

	
	
	2
	BMW 2004 Reg. B 2
	Ballast water operation was not entered into the rec. book immediately upon completion.Master instructed to keep proper records from now.

	
	
	3
	SOLAS III Reg. 20
	Embarkation ladder (both sides) side ropes found frayed and weakened.

	
	
	4
	SOLAS V Reg. 23
	Pilot ladder found deformed frayed and weakened.

	
	

17.08.2026
	
1
	SOLAS II-2 Reg. 14.2
	Observed small leakage from fire hydrant on fwd port side of the vessel.

	
	
	2
	MLC 2006 Title 4 Std. A 4.3
	Two grinders in forecastle found without protection wheel guard.

	
	
	
	
	

	
SIBENIK
	

05.05.2026
	1
	ICLL Art.15
	Hatch coaming corroded.

	
	
	2
	ICLL Reg.16
	Pontoon hatch covers rubber gaskets, pontoons no 4,5,6 damaged.

	
	
	3
	MLC 2006 Title 4 Reg. 4.3
	Bow thruster engine oil leakage found.




